DSan Video Clock for Limitimer Version 75

Use this application to display data from LIMITIMER ONLY using the appropriate VC-2000 USB--Cat-5 dongle.

If the installation stops midway, that mean that you may have to disable your anti-virus software to load this application.

This set up program will load the Video Clock files into your Program Files directory under DSAN-Video Clock subdirectory.

You may select any other directory and run the executable from that directory.    The program looks for bitmap files located in directories relative to the location of the application executable.

No files are added to the Windows System directory.  All application files are placed in the Video Clock installation directory.  When you save a configuration, a registry entry is made uner Local Machine | Software | DSAN.  This tells the application to open this configuration the next time it is launched.

Use this application to display LIMITIMER  DATA ONLY.  Please request a different dongle and different software to display data from other DSan products such as The Deliberator and PerfectCue.  Each dongle can display date from one product.  Only one instance of the program can run at one time.

The uninstall facility deletes all files associated with the application from your computer except those file and images that you have created.

Questions and answers as well as other resources are available at www.dsan.com/VideoClock.

Refer to the User Guide via a shortcut link on the Start | All Programs menu under DSAN- Video Clock 

This application makes extensive use of Windows components available only in the libraries found when the Visual C++ development tool, Visual Studio,  has been installed.   To install these components on your machine (without installing Visual Studio), please visit Microsoft at 

https://www.microsoft.com/en-us/download/details.aspx?id=48145

The configuration files included are set to Read Only.  Save your own custom configurations with other file names.

If you are connected to the Internet, you may see the Time Remaining counting down and the bitmaps representing Green-Yellow-Red phase lights switch.  That is becauase the configurations are set to receive data from a Limitimer data stream running from our office at IP address: 47.23.6.155 Port: 64444.  You will need to set the data interface to "USB" for connection to your timer.

DSan Corporation
516 625-5608
sales@dsan.com